{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["BOM(请将需要匹配的BOM放在第一个工作表即sheet1）","Please put the BOM to sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOM(请将需要匹配的BOM放在第一个工作表即sheet1）","index":0,"n_rows":12,"n_cols":9,"rows_kept":12,"flags":["formulas_cached_only"]}
["序号","产品分类","品牌","型号*","规格参数描述*","封装*","位号*","单机用量*","备注"]
[1,"贴片电容","FH","0402B103K250NT","25V 10nF",402,"C3,C4,C5,C6",4]
[2,"贴片电容","Samsung","CL05B104K05NNNC","16V 100nF",402,"C1,C2,",2]
[3,"肖特基二极管","MDD","1N5819",null,"SOD-323","D1,D2",2]
[4,"IC","ROHM","BR24L08FV-WE2",null,null,"U3",1]
[5,"IC","ROHM","BR34E02FVT-3E2",null,null,"U2, U3",2]
[6,"贴片电阻","UniOhm","0402WGF330JTCE","33Ω",402,"R4",1]
[7,"贴片电阻","Uniohm","0402WGF1001TCE","1KΩ",402,"R1,R2,R3,R4",4]
[8,"贴片电阻","UniOhm","0603WAJ0105T5E","1MΩ",603,"R5",1]
[9,"贴片电阻","Walsin","WR06X225JTL","2.2MΩ",603,"R37",1]
[10,"贴片电阻","RALEC","RTT03102JTP","1KΩ",603,"R46",1]
[11,"二极管","MCC","1N4148W-TP",null,"SOD123","D3",1]

{"sheet":"Please put the BOM to sheet1","index":1,"n_rows":12,"n_cols":9,"rows_kept":12,"flags":["formulas_cached_only"]}
["序号","产品分类","品牌","型号*","规格参数描述*","封装*","位号*","单机用量*","备注"]
[1,"The patch capacitance ","FH","0402B103K250NT","25V 10nF",402,"C3,C4,C5,C6",4]
[2,"The patch capacitance ","Samsung","CL05B104K05NNNC","16V 100nF",402,"C1,C2,",2]
[3,"Schottky diode","MDD","1N5819",null,"SOD-323","D1,D2",2]
[4,"IC","ROHM","BR24L08FV-WE2",null,null,"U3",1]
[5,"IC","ROHM","BR34E02FVT-3E2",null,null,"U2, U3",2]
[6,"SMD resistor ","UniOhm","0402WGF330JTCE","33Ω",402,"R4",1]
[7,"SMD resistor ","Uniohm","0402WGF1001TCE","1KΩ",402,"R1,R2,R3,R4",4]
[8,"SMD resistor ","UniOhm","0603WAJ0105T5E","1MΩ",603,"R5",1]
[9,"SMD resistor ","Walsin","WR06X225JTL","2.2MΩ",603,"R37",1]
[10,"SMD resistor","RALEC","RTT03102JTP","1KΩ",603,"R46",1]
[11,"diode","MCC","1N4148W-TP",null,"SOD123","D3",1]